After running and recording several instances( 12 total recorded) I stumbled upon a few interesting results. I noticed that cache line size directly correlates to the speed of the cache, more so than the memory size itself. I also noticed that having a faster cache access time is much more influential than having a fast memory access time. The hit ratio was also significantly higher ~10%, when using larger line sizes than with smaller.